U A

0 25 50 75 100 125 150 175 200

0 25 50 75 100 125 150 175 200

-20 -15 -10 -5 0 5 10 15

0 25 50 75 100 125 150 175 200

FCal only, 80 GeV calibration, no noise cut

FCal+TC, FCal 80 GeV, TC 200 GeV TC calib., no noise cut

FCal only, 80 GeV calibration, no noise cut

FCal+TC, FCal 80 GeV, TC 200 GeV TC calib., no noise cut

FCal only, 80 GeV calibration, 2σ noise cut

FCal Pion Signal Linearity

Beam Energy [GeV]

Deviation from Linearity [%]

Reconstructed Energy [GeV]

* FCal signals calibrated at 80 GeV (with/without noise cut) * TC signal calibrated at 200 GeV (no noise cut) * average signal reconstructed from Gaussian fits to FCal and FCal+TC signal distributions