U A

Beam Particle Trigger (3 Scintillator Counters)

S1 S3 S2

Multi-Wire Proportional Chambers (1 x, 1 y plane each)

Veto System (Scintillator Veto Wall and Hole Veto)

Beamline

(Particle Trigger, Position and Direction Measurement)

z y

Concrete Beam Stop

Muon Counter (Scintillator)

Tail Catcher (Iron/Scintillator Calorimeter)

Low Density Argon Excluder

Forward Calorimeter Modules

1 2

Liquid Argon Cryostat

Test Area

(Calorimeter Modules, Leakage Detectors, Particle Identification)