U A Not to scale!

η = 3.7

50% lateral containment (pions, 100 GeV)

FCal1 Module 0 (front)

FCal2 Module 0 (back)

80% containment

90% containment

r = 15 cm

bi-gain readout for shaded tiles!

FCal Module 0 ReadOut

η = 3.7

r = 15 cm

# tiles: 192 # channels: 256 bi-gain: 64

# tiles: 128 # channels: 160 bi-gain: 32

beam spot ~5 cm O